SEND "INPUT-1"
ICHR 1 00
SEND "INPUT-2"
ICHR 2 01
CMPM 00 01 AAA
SEND "OK"
GOTO BBB
:AAA
SEND "NG"
:BBB
SEND "1+2="
MADD 00 01
MSED 00
SEND "CHACKSAM"
CHKA 01 02
MSED 02
CHKH 01 03
MSED 03
PUSE 1 CCC
SEND "1-ON"
GOTO DDD
:CCC
SEND "1-OFF"
:DDD
PUSM 04
CMPL 04 EEE "002"
SEND "2-ON"
GOTO FFF
:EEE
SEND "2-OFF"
:FFF
SEND "TEST-END"
PEND
